INVITATION TO BID


Sealed proposals for:	

Contractor* for lower-level Firehouse repair (post-flood damage)

*Must be licensed & insured and show proof of such. 

Scope of work: See attached.
 
Will be received by:

GREENVILLE FIRE DISTRICT
711 CENTRAL PARK AVENUE
SCARSDALE, NY 10583

Proposals must be received on or before 12:00 Noon, local time, on Tuesday, August 18, 2026 and must be in accordance with the requirements of the bidding documents to receive consideration.  Bids will be opened at this location at 1:00 P.M., local time, on Friday, August 7, 2026.

[bookmark: _Hlk200452362][bookmark: _Hlk200452371]Specifications / walk-through for this project will be available upon request beginning on Friday, August 7, 2026: 
			
At the offices of:		GREENVILLE FIRE DISTRICT
711 CENTRAL PARK AVENUE
SCARSDALE, NY 10583

This information will also be available on the Greenville Fire District Website:   www.fdgreenville.com. 

Site visits can be scheduled by emailing Deputy Treasurer, Jennifer DiMartino at Jen@fdgreenville.com

[bookmark: _Hlk200452474]Proposals must be submitted in sealed envelopes bearing on the outside the name and address of the bidder and the name of the project name (Contractor for lower-level Firehouse repair (post-flood damage)).

All bid prices shall be filled in, both with words and figures.  Signatures shall be in ink and in longhand.  Proposals which are incomplete, conditional or obscure may be rejected as informal. 

No oral or telephonic proposals or modification of proposals will be considered.  Addenda, if any, issued before submission of bids, shall be taken into account if included in the proposal.  

JENNIFER L. DIMARTINO
DEPUTY TREASURER / SECRETARY   
BOARD OF FIRE COMMISSIONERS
GREENVILLE FIRE DISTRICT
TOWN OF GREENBURGH
WESTCHESTER COUNTY, NY
August 6, 2026


Scope of work:

Drywall Repair
Provide labor, materials to install new 5/8" drywall in the currently opened lower-wall areas of the designated lower level. Interior partition walls to receive two layers of 5/8" drywall, with the concealed layer hung and fire-taped and the exposed layer fully taped, finished, sanded, and prepared for paint. Exterior perimeter walls to receive one layer of 5/8" drywall, fully finished and prepared for paint. New drywall will terminate above the existing approximately 6" epoxy-coated drywall base, which is to remain, with continuous trim installed over the transition. Includes fasteners, cutouts, corner bead, joint compound, material handling, protection, and cleanup.

Painting
Provide labor, materials to prepare and paint all designated drywall wall surfaces within the lower-level work areas. Scope includes spot preparation as required, one full coat of drywall primer, and two finish coats of interior wall paint. Paint all associated base trim within the designated areas.
Includes protection of adjacent floors, doors, fixtures, equipment, and finishes, along with cleanup and disposal of painting-related debris.
Excludes: Ceilings, masonry walls, concrete surfaces, doors, door frames, cabinets, exposed piping, equipment, and any surfaces not specifically identified as drywall walls or base trim.

Door Restoration and Painting
Sand and prepare five existing interior wood doors affected by flood water. Clean and remove visible mildew and staining, treat affected areas, and apply new stain to restore a uniform appearance.

Ceiling Tiles
Repair approximately 24' × 5' area of damaged suspended ceiling. Remove damaged ceiling tiles and grid components, repair or replace affected main runners, cross tees, hanger wires, and perimeter molding as required, and install new matching ceiling tiles.


